

Read/Write File Transfer

|  |  |  |
| --- | --- | --- |
| C1: Form DATA packet (with DATA or ACK)  C2: Create Datagram w/ TFTP DATA Packet  C3: Send Datagram  C4: Wait & Receive Response  C5: Extract Message  C6: Output Message | E1: Wait & Receive DATA Packet  E2: Extract Message  E3: Form DATA Packet  E4: Send DATA Packet  E5: Wait & Receive Response  E6: Extract Message  E7: Form DATA Packet  E8: Send DATA Packet | S1: Receive Datagram  S1: Extract UDP Datagram  S3: Handle Request Type (Check if need to ACK)  S4: Form Datagram  S5: Send Datagram  S6: Receive Datagram  S7: Extract Message (Path after ACK0) |